<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="62.23" y2="0" width="0" layer="20"/>
<wire x1="62.23" y1="0" x2="63.5" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="63.5" y1="1.27" x2="63.5" y2="36.83" width="0" layer="20"/>
<wire x1="63.5" y1="36.83" x2="62.23" y2="38.1" width="0" layer="20" curve="90"/>
<wire x1="62.23" y1="38.1" x2="1.27" y2="38.1" width="0" layer="20"/>
<wire x1="1.27" y1="38.1" x2="0" y2="36.83" width="0" layer="20" curve="90"/>
<wire x1="0" y1="36.83" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>VCC</text>
<text>GND</text>
<text>VCC</text>
<text>Off</text>
<text>On</text>
<text>AASaver v2.0</text>
<text>Flash Led</text>
<text>http://rayshobby.net</text>
<text>On</text>
<text>Off</text>
<text>On</text>
<text>Lipo</text>
<text>Lipo</text>
<text>CHG</text>
<text>GND</text>
<text>VCC</text>
<hole x="31" y="31" drill="3"/>
<hole x="31" y="15" drill="2.8"/>
<text>Out</text>
<text>In</text>
<text>VCC</text>
<text>GND</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>Source</text>
<text>Lipo</text>
<text>AA</text>
<text>Charge</text>
<text>200mA</text>
<text>10mA</text>
<text>Current</text>
<text>20mA</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>VCC</text>
</plain>
<libraries>
<library name="resistor">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X02_BIG">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="CR75">
</package>
<package name="DO216AA-DIODE">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="TC33X">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFunNew">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-S-FEMALE">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="EIA7343">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT236">
</package>
</packages>
</library>
<library name="adafruitGood">
<packages>
<package name="EG1213">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFunNew" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP0" library="SparkFun" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1'" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="PWR" library="led" package="CHIPLED_0805" value="red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="1.5K">
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFunNew" package="USB-A-S-FEMALE" value="USB-A-S-FEMALE"/>
<element name="C5" library="SparkFunNew" package="EIA3216" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MCP" library="SparkFunNew" package="SOT23-5" value="MCP73831">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="1.5K">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_0805" value="green">
<attribute name="VALUE"/>
</element>
<element name="C4" library="resistor" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RCHG" library="rcl" package="R0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFunNew" package="AYZ0202" value="AYZ0202"/>
<element name="J3" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J0" library="SparkFunNew" package="AYZ0202" value="AYZ0202">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="POT" library="adafruit" package="TC33X" value="100K">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT236" value="NTGS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun" package="CR75" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NCP" library="SparkFunNew" package="SOT23-5" value="NCP1450A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun" package="DO216AA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="resistor" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFunNew" package="EIA7343" value="220uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT+" library="rcl" package="R0805" value="75K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB+" library="rcl" package="R0805" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT-" library="rcl" package="R0805" value="75K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB-" library="rcl" package="R0805" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="1X02_BIG" value=""/>
<element name="S1" library="adafruitGood" package="EG1213" value="EG1213"/>
<element name="JP3" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP0" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="X1" pad="GND"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="NCP" pad="4"/>
<contactref element="Q1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="C"/>
<contactref element="RB+" pad="1"/>
<contactref element="RB-" pad="1"/>
<contactref element="JP5" pad="P$2"/>
<contactref element="MCP" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="POT" pad="3"/>
<contactref element="C5" pad="C"/>
<contactref element="S1" pad="MT1"/>
<contactref element="S1" pad="MT2"/>
<contactref element="JP4" pad="1"/>
<contactref element="C1" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="RT+" pad="2"/>
<contactref element="RT-" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP0" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="MCP" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="J0" pad="2"/>
<contactref element="J0" pad="5"/>
<contactref element="C3" pad="A"/>
<contactref element="NCP" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="D4" pad="C"/>
<contactref element="PWR" pad="A"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="2"/>
<contactref element="LED1'" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="PWR" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="LED3" pad="C"/>
<contactref element="MCP" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="MCP" pad="5"/>
<contactref element="RCHG" pad="2"/>
</signal>
<signal name="VCHGOUT">
<contactref element="MCP" pad="3"/>
<contactref element="MCP" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="C5" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="POT" pad="2"/>
<contactref element="RCHG" pad="1"/>
</signal>
<signal name="D+">
<contactref element="X1" pad="D+"/>
<contactref element="RT+" pad="1"/>
<contactref element="RB+" pad="2"/>
</signal>
<signal name="D-">
<contactref element="X1" pad="D-"/>
<contactref element="RT-" pad="1"/>
<contactref element="RB-" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="L1" pad="P$1"/>
<contactref element="NCP" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="J0" pad="6"/>
<contactref element="J0" pad="3"/>
<contactref element="LED1'" pad="A"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="NCP" pad="5"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="6"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="3"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
